Product Details

**Introduction:**

FR4 100 is a long strip of UHF passive RFID tag, the chip is NXP G2XM and G2XL, using the high temperature resistant RF4 high-performance insulation base material, this tag outstanding features can be used in any medium surface, such as metal, wood and air, can be normal installation and use.

**Specification:**

**Chip Available: G2XM, G2XL  
Communication protocol: UHF EPC G2  
Frequency: 915MHz (can be 860-960MHz)   
Operating temperature: -20℃-140℃  
Distance: 4m (9dbi antenna)  
Standard Color: Black  
Material: FR4  
Size: 100×11×3mm , 113×16.5×3mm , 138×22×3mm**

**Other Features:**

**Storage temperature: -30℃-160℃**

**Can be installed in different object (metal, walls and board), logistics, petrol, asset management etc,**

**and can be resisted high temperature, prevent moisture, corrosion resistance, suitable for bad environment.**

****